The computer has two USB4 ports, coded as 80 and 84 respectively, so you need to update twice. After the update is complete, select the other port and repeat the steps below.

1.Click GetVersion to get the current USB4 firmware version

2.Click Load BinFile, select the new firmware file -- Maita NUCAL02 IT8856 Test VF0310

3.Click Update FW to start flashing the USB4 firmware

4.After the update is complete, click GetVersion again to retrieve the current USB4 firmware version, and confirm if it is F010. If so, it indicates that the update was successful.

5.After both interfaces have been updated, shut down the computer, unplug it, and restart to complete the process thoroughly.