## Summary

Report Date | 2017-01-01 00:05:31
Generated by | MemTest86 V7.5 Free (64-bit)
Result | FAIL

## System Information

EFI Specifications | 2.70
System |
Manufacturer | Default string
Product Name | Default string
Version | Default string
Serial Number | Default string
BIOS |
Vendor | American Megatrends Inc.
Version | V0.51_P2C2M3_Jinhua_X8_tRef_DoubleEn
Release Date | 04/21/2020
Baseboard |
Manufacturer | Default string
Product Name | Default string
Version | Default string
Serial Number | Default string
CPU Type | AMD Athlon 300U with Radeon Vega Mobile Gfx
CPU Clock | 2406 MHz [Turbo: 3308.0 MHz]
# Logical Processors | 4
L1 Cache | 4 x 96K (77011 MB/s)
L2 Cache | 4 x 512K (56366 MB/s)
L3 Cache | 1 x 4096K (19301 MB/s)
Memory | 6100M (14971 MB/s)
DIMM Slot #0 | 4GB DDR4 PC4-19200
| Unknown / CA4S4G08V-F7GNC-4
| 2400 MHz
DIMM Slot #1 | 4GB DDR4 PC4-19200
| Unknown / CA4S4G08V-F7GNC-4
| 2400 MHz

## Result summary

Test Start Time | 2017-01-01 00:02:30
Elapsed Time | 0:00:49
Memory Range Tested | 0x0 - 220000000 (8704MB)
CPU Selection Mode | Parallel (All CPUs)
ECC Polling | Enabled
# Tests Passed | 1/4 (25%)

Lowest Error Address | 0x566AA640 (1382MB)
Highest Error Address | 0x216D4BEB0 (8557MB)
Bits in Error Mask | 0000000000005B00
Bits in Error | 5
Max Contiguous Errors | 1

Test | # Tests Passed | Errors
Test 0 [Address test, walking ones, 1 CPU] | 1/1 (100%) | 0
Test 1 [Address test, own address, 1 CPU] | 0/1 (0%) | 19
Test 2 [Address test, own address] | 0/1 (0%) | 58
Test 3 [Moving inversions, ones & zeroes] | 0/1 (0%) | 1619
Test 4 [Moving inversions, 8-bit pattern] | 0/0 (0%) | 8389
Test 5 [Moving inversions, random pattern] | 0/0 (0%) | 0
Test 6 [Block move, 64-byte blocks] | 0/0 (0%) | 0
Test 7 [Moving inversions, 32-bit pattern] | 0/0 (0%) | 0
Test 8 [Random number sequence] | 0/0 (0%) | 0
Test 9 [Modulo 20, ones & zeros] | 0/0 (0%) | 0
Test 10 [Bit fade test, 2 patterns, 1 CPU] | 0/0 (0%) | 0
Test 13 [Hammer test] | 0/0 (0%) | 0

Last 10 Errors
[Data Error] Test: 4, CPU: 1, Address: 120BD6A10, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 2, Address: 124B56C10, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 3, Address: 128B56A10, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 1, Address: 120B56E10, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 3, Address: 128A96410, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 1, Address: 120A96010, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 3, Address: 128A16010, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 3, Address: 1289D7E10, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 3, Address: 128997C10, Expected: 80808080, Actual: 8080C080
[Data Error] Test: 4, CPU: 1, Address: 120A16410, Expected: 80808080, Actual: 8080C080

## Certification